   1              		.cpu cortex-m4
   2              		.eabi_attribute 27, 1
   3              		.eabi_attribute 28, 1
   4              		.eabi_attribute 20, 1
   5              		.eabi_attribute 21, 1
   6              		.eabi_attribute 23, 3
   7              		.eabi_attribute 24, 1
   8              		.eabi_attribute 25, 1
   9              		.eabi_attribute 26, 1
  10              		.eabi_attribute 30, 6
  11              		.eabi_attribute 34, 1
  12              		.eabi_attribute 18, 4
  13              		.file	"startup_msp432p401r_gcc.c"
  14              		.text
  15              	.Ltext0:
  16              		.cfi_sections	.debug_frame
  17              		.comm	component_fun,4,4
  18              		.global	interruptVectors
  19              		.section	.intvecs,"a",%progbits
  20              		.align	2
  23              	interruptVectors:
  24 0000 00000000 		.word	__StackTop
  25 0004 00000000 		.word	Reset_Handler
  26 0008 00000000 		.word	NMI_Handler
  27 000c 00000000 		.word	HardFault_Handler
  28 0010 00000000 		.word	MemManage_Handler
  29 0014 00000000 		.word	BusFault_Handler
  30 0018 00000000 		.word	UsageFault_Handler
  31 001c 00000000 		.word	0
  32 0020 00000000 		.word	0
  33 0024 00000000 		.word	0
  34 0028 00000000 		.word	0
  35 002c 00000000 		.word	SVC_Handler
  36 0030 00000000 		.word	DebugMon_Handler
  37 0034 00000000 		.word	0
  38 0038 00000000 		.word	PendSV_Handler
  39 003c 00000000 		.word	SysTick_Handler
  40 0040 00000000 		.word	PSS_IRQHandler
  41 0044 00000000 		.word	CS_IRQHandler
  42 0048 00000000 		.word	PCM_IRQHandler
  43 004c 00000000 		.word	WDT_A_IRQHandler
  44 0050 00000000 		.word	FPU_IRQHandler
  45 0054 00000000 		.word	FLCTL_IRQHandler
  46 0058 00000000 		.word	COMP_E0_IRQHandler
  47 005c 00000000 		.word	COMP_E1_IRQHandler
  48 0060 00000000 		.word	TA0_0_IRQHandler
  49 0064 00000000 		.word	TA0_N_IRQHandler
  50 0068 00000000 		.word	TA1_0_IRQHandler
  51 006c 00000000 		.word	TA1_N_IRQHandler
  52 0070 00000000 		.word	TA2_0_IRQHandler
  53 0074 00000000 		.word	TA2_N_IRQHandler
  54 0078 00000000 		.word	TA3_0_IRQHandler
  55 007c 00000000 		.word	TA3_N_IRQHandler
  56 0080 00000000 		.word	EUSCIA0_IRQHandler
  57 0084 00000000 		.word	EUSCIA1_IRQHandler
  58 0088 00000000 		.word	EUSCIA2_IRQHandler
  59 008c 00000000 		.word	EUSCIA3_IRQHandler
  60 0090 00000000 		.word	EUSCIB0_IRQHandler
  61 0094 00000000 		.word	EUSCIB1_IRQHandler
  62 0098 00000000 		.word	EUSCIB2_IRQHandler
  63 009c 00000000 		.word	EUSCIB3_IRQHandler
  64 00a0 00000000 		.word	ADC14_IRQHandler
  65 00a4 00000000 		.word	T32_INT1_IRQHandler
  66 00a8 00000000 		.word	T32_INT2_IRQHandler
  67 00ac 00000000 		.word	T32_INTC_IRQHandler
  68 00b0 00000000 		.word	AES256_IRQHandler
  69 00b4 00000000 		.word	RTC_C_IRQHandler
  70 00b8 00000000 		.word	DMA_ERR_IRQHandler
  71 00bc 00000000 		.word	DMA_INT3_IRQHandler
  72 00c0 00000000 		.word	DMA_INT2_IRQHandler
  73 00c4 00000000 		.word	DMA_INT1_IRQHandler
  74 00c8 00000000 		.word	DMA_INT0_IRQHandler
  75 00cc 00000000 		.word	PORT1_IRQHandler
  76 00d0 00000000 		.word	PORT2_IRQHandler
  77 00d4 00000000 		.word	PORT3_IRQHandler
  78 00d8 00000000 		.word	PORT4_IRQHandler
  79 00dc 00000000 		.word	PORT5_IRQHandler
  80 00e0 00000000 		.word	PORT6_IRQHandler
  81              		.text
  82              		.align	1
  83              		.weak	Reset_Handler
  84              		.syntax unified
  85              		.thumb
  86              		.thumb_func
  87              		.fpu fpv4-sp-d16
  89              	Reset_Handler:
  90              	.LFB123:
  91              		.file 1 "srcc/startup_msp432p401r_gcc.c"
   1:srcc/startup_msp432p401r_gcc.c **** /******************************************************************************
   2:srcc/startup_msp432p401r_gcc.c **** * 
   3:srcc/startup_msp432p401r_gcc.c **** *  Copyright (C) 2012 - 2016 Texas Instruments Incorporated - http://www.ti.com/ 
   4:srcc/startup_msp432p401r_gcc.c **** * 
   5:srcc/startup_msp432p401r_gcc.c **** *  Redistribution and use in source and binary forms, with or without 
   6:srcc/startup_msp432p401r_gcc.c **** *  modification, are permitted provided that the following conditions 
   7:srcc/startup_msp432p401r_gcc.c **** *  are met:
   8:srcc/startup_msp432p401r_gcc.c **** * 
   9:srcc/startup_msp432p401r_gcc.c **** *   Redistributions of source code must retain the above copyright 
  10:srcc/startup_msp432p401r_gcc.c **** *   notice, this list of conditions and the following disclaimer.
  11:srcc/startup_msp432p401r_gcc.c **** * 
  12:srcc/startup_msp432p401r_gcc.c **** *   Redistributions in binary form must reproduce the above copyright
  13:srcc/startup_msp432p401r_gcc.c **** *   notice, this list of conditions and the following disclaimer in the 
  14:srcc/startup_msp432p401r_gcc.c **** *   documentation and/or other materials provided with the   
  15:srcc/startup_msp432p401r_gcc.c **** *   distribution.
  16:srcc/startup_msp432p401r_gcc.c **** * 
  17:srcc/startup_msp432p401r_gcc.c **** *   Neither the name of Texas Instruments Incorporated nor the names of
  18:srcc/startup_msp432p401r_gcc.c **** *   its contributors may be used to endorse or promote products derived
  19:srcc/startup_msp432p401r_gcc.c **** *   from this software without specific prior written permission.
  20:srcc/startup_msp432p401r_gcc.c **** * 
  21:srcc/startup_msp432p401r_gcc.c **** *  THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS 
  22:srcc/startup_msp432p401r_gcc.c **** *  "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT 
  23:srcc/startup_msp432p401r_gcc.c **** *  LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR
  24:srcc/startup_msp432p401r_gcc.c **** *  A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT 
  25:srcc/startup_msp432p401r_gcc.c **** *  OWNER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, 
  26:srcc/startup_msp432p401r_gcc.c **** *  SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT 
  27:srcc/startup_msp432p401r_gcc.c **** *  LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE,
  28:srcc/startup_msp432p401r_gcc.c **** *  DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY
  29:srcc/startup_msp432p401r_gcc.c **** *  THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT 
  30:srcc/startup_msp432p401r_gcc.c **** *  (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE 
  31:srcc/startup_msp432p401r_gcc.c **** *  OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.  
  32:srcc/startup_msp432p401r_gcc.c **** * 
  33:srcc/startup_msp432p401r_gcc.c **** *  MSP432P401R Interrupt Vector Table
  34:srcc/startup_msp432p401r_gcc.c **** * 
  35:srcc/startup_msp432p401r_gcc.c **** *****************************************************************************/
  36:srcc/startup_msp432p401r_gcc.c **** 
  37:srcc/startup_msp432p401r_gcc.c **** #include <stdint.h>
  38:srcc/startup_msp432p401r_gcc.c **** #include "msp432p401r.h"
  39:srcc/startup_msp432p401r_gcc.c **** #include "user.h"
  40:srcc/startup_msp432p401r_gcc.c **** 
  41:srcc/startup_msp432p401r_gcc.c **** /* Entry point for the application. */
  42:srcc/startup_msp432p401r_gcc.c **** extern int main(void);
  43:srcc/startup_msp432p401r_gcc.c **** 
  44:srcc/startup_msp432p401r_gcc.c **** /* External declaration for system initialization function                  */
  45:srcc/startup_msp432p401r_gcc.c **** extern void SystemInit(void);
  46:srcc/startup_msp432p401r_gcc.c **** 
  47:srcc/startup_msp432p401r_gcc.c **** extern uint32_t __data_load__;
  48:srcc/startup_msp432p401r_gcc.c **** extern uint32_t __data_start__;
  49:srcc/startup_msp432p401r_gcc.c **** extern uint32_t __data_end__;
  50:srcc/startup_msp432p401r_gcc.c **** extern uint32_t __StackTop;
  51:srcc/startup_msp432p401r_gcc.c **** 
  52:srcc/startup_msp432p401r_gcc.c **** typedef void( *pFunc )( void );
  53:srcc/startup_msp432p401r_gcc.c **** //extern void  BIOS_API_Init();
  54:srcc/startup_msp432p401r_gcc.c **** /* Forward declaration of the default fault handlers. */
  55:srcc/startup_msp432p401r_gcc.c **** void Default_Handler(void);
  56:srcc/startup_msp432p401r_gcc.c **** extern void Reset_Handler       (void) __attribute__((weak));
  57:srcc/startup_msp432p401r_gcc.c **** 
  58:srcc/startup_msp432p401r_gcc.c **** /* Cortex-M4 Processor Exceptions */
  59:srcc/startup_msp432p401r_gcc.c **** extern void NMI_Handler         (void) __attribute__((weak, alias("Default_Handler")));
  60:srcc/startup_msp432p401r_gcc.c **** extern void HardFault_Handler   (void) __attribute__((weak, alias("Default_Handler")));
  61:srcc/startup_msp432p401r_gcc.c **** extern void MemManage_Handler   (void) __attribute__((weak, alias("Default_Handler")));
  62:srcc/startup_msp432p401r_gcc.c **** extern void BusFault_Handler    (void) __attribute__((weak, alias("Default_Handler")));
  63:srcc/startup_msp432p401r_gcc.c **** extern void UsageFault_Handler  (void) __attribute__((weak, alias("Default_Handler")));
  64:srcc/startup_msp432p401r_gcc.c **** extern void SVC_Handler         (void) __attribute__((weak, alias("Default_Handler")));
  65:srcc/startup_msp432p401r_gcc.c **** extern void DebugMon_Handler    (void) __attribute__((weak, alias("Default_Handler")));
  66:srcc/startup_msp432p401r_gcc.c **** extern void PendSV_Handler      (void) __attribute__((weak, alias("Default_Handler")));
  67:srcc/startup_msp432p401r_gcc.c **** 
  68:srcc/startup_msp432p401r_gcc.c **** /* device specific interrupt handler */
  69:srcc/startup_msp432p401r_gcc.c **** extern void SysTick_Handler     (void) __attribute__((weak,alias("Default_Handler")));
  70:srcc/startup_msp432p401r_gcc.c **** extern void PSS_IRQHandler      (void) __attribute__((weak,alias("Default_Handler")));
  71:srcc/startup_msp432p401r_gcc.c **** extern void CS_IRQHandler       (void) __attribute__((weak,alias("Default_Handler")));
  72:srcc/startup_msp432p401r_gcc.c **** extern void PCM_IRQHandler      (void) __attribute__((weak,alias("Default_Handler")));
  73:srcc/startup_msp432p401r_gcc.c **** extern void WDT_A_IRQHandler    (void) __attribute__((weak,alias("Default_Handler")));
  74:srcc/startup_msp432p401r_gcc.c **** extern void FPU_IRQHandler      (void) __attribute__((weak,alias("Default_Handler")));
  75:srcc/startup_msp432p401r_gcc.c **** extern void FLCTL_IRQHandler    (void) __attribute__((weak,alias("Default_Handler")));
  76:srcc/startup_msp432p401r_gcc.c **** extern void COMP_E0_IRQHandler  (void) __attribute__((weak,alias("Default_Handler")));
  77:srcc/startup_msp432p401r_gcc.c **** extern void COMP_E1_IRQHandler  (void) __attribute__((weak,alias("Default_Handler")));
  78:srcc/startup_msp432p401r_gcc.c **** extern void TA0_0_IRQHandler    (void) __attribute__((weak,alias("Default_Handler")));
  79:srcc/startup_msp432p401r_gcc.c **** extern void TA0_N_IRQHandler    (void) __attribute__((weak,alias("Default_Handler")));
  80:srcc/startup_msp432p401r_gcc.c **** extern void TA1_0_IRQHandler    (void) __attribute__((weak,alias("Default_Handler")));
  81:srcc/startup_msp432p401r_gcc.c **** extern void TA1_N_IRQHandler    (void) __attribute__((weak,alias("Default_Handler")));
  82:srcc/startup_msp432p401r_gcc.c **** extern void TA2_0_IRQHandler    (void) __attribute__((weak,alias("Default_Handler")));
  83:srcc/startup_msp432p401r_gcc.c **** extern void TA2_N_IRQHandler    (void) __attribute__((weak,alias("Default_Handler")));
  84:srcc/startup_msp432p401r_gcc.c **** extern void TA3_0_IRQHandler    (void) __attribute__((weak,alias("Default_Handler")));
  85:srcc/startup_msp432p401r_gcc.c **** extern void TA3_N_IRQHandler    (void) __attribute__((weak,alias("Default_Handler")));
  86:srcc/startup_msp432p401r_gcc.c **** extern void EUSCIA0_IRQHandler  (void) __attribute__((weak,alias("Default_Handler")));
  87:srcc/startup_msp432p401r_gcc.c **** extern void EUSCIA1_IRQHandler  (void) __attribute__((weak,alias("Default_Handler")));
  88:srcc/startup_msp432p401r_gcc.c **** extern void EUSCIA2_IRQHandler  (void) __attribute__((weak,alias("Default_Handler")));
  89:srcc/startup_msp432p401r_gcc.c **** extern void EUSCIA3_IRQHandler  (void) __attribute__((weak,alias("Default_Handler")));
  90:srcc/startup_msp432p401r_gcc.c **** extern void EUSCIB0_IRQHandler  (void) __attribute__((weak,alias("Default_Handler")));
  91:srcc/startup_msp432p401r_gcc.c **** extern void EUSCIB1_IRQHandler  (void) __attribute__((weak,alias("Default_Handler")));
  92:srcc/startup_msp432p401r_gcc.c **** extern void EUSCIB2_IRQHandler  (void) __attribute__((weak,alias("Default_Handler")));
  93:srcc/startup_msp432p401r_gcc.c **** extern void EUSCIB3_IRQHandler  (void) __attribute__((weak,alias("Default_Handler")));
  94:srcc/startup_msp432p401r_gcc.c **** extern void ADC14_IRQHandler    (void) __attribute__((weak,alias("Default_Handler")));
  95:srcc/startup_msp432p401r_gcc.c **** extern void T32_INT1_IRQHandler (void) __attribute__((weak,alias("Default_Handler")));
  96:srcc/startup_msp432p401r_gcc.c **** extern void T32_INT2_IRQHandler (void) __attribute__((weak,alias("Default_Handler")));
  97:srcc/startup_msp432p401r_gcc.c **** extern void T32_INTC_IRQHandler (void) __attribute__((weak,alias("Default_Handler")));
  98:srcc/startup_msp432p401r_gcc.c **** extern void AES256_IRQHandler   (void) __attribute__((weak,alias("Default_Handler")));
  99:srcc/startup_msp432p401r_gcc.c **** extern void RTC_C_IRQHandler    (void) __attribute__((weak,alias("Default_Handler")));
 100:srcc/startup_msp432p401r_gcc.c **** extern void DMA_ERR_IRQHandler  (void) __attribute__((weak,alias("Default_Handler")));
 101:srcc/startup_msp432p401r_gcc.c **** extern void DMA_INT3_IRQHandler (void) __attribute__((weak,alias("Default_Handler")));
 102:srcc/startup_msp432p401r_gcc.c **** extern void DMA_INT2_IRQHandler (void) __attribute__((weak,alias("Default_Handler")));
 103:srcc/startup_msp432p401r_gcc.c **** extern void DMA_INT1_IRQHandler (void) __attribute__((weak,alias("Default_Handler")));
 104:srcc/startup_msp432p401r_gcc.c **** extern void DMA_INT0_IRQHandler (void) __attribute__((weak,alias("Default_Handler")));
 105:srcc/startup_msp432p401r_gcc.c **** extern void PORT1_IRQHandler    (void) __attribute__((weak,alias("Default_Handler")));
 106:srcc/startup_msp432p401r_gcc.c **** extern void PORT2_IRQHandler    (void) __attribute__((weak,alias("Default_Handler")));
 107:srcc/startup_msp432p401r_gcc.c **** extern void PORT3_IRQHandler    (void) __attribute__((weak,alias("Default_Handler")));
 108:srcc/startup_msp432p401r_gcc.c **** extern void PORT4_IRQHandler    (void) __attribute__((weak,alias("Default_Handler")));
 109:srcc/startup_msp432p401r_gcc.c **** extern void PORT5_IRQHandler    (void) __attribute__((weak,alias("Default_Handler")));
 110:srcc/startup_msp432p401r_gcc.c **** extern void PORT6_IRQHandler    (void) __attribute__((weak,alias("Default_Handler")));
 111:srcc/startup_msp432p401r_gcc.c **** 
 112:srcc/startup_msp432p401r_gcc.c **** /* Interrupt vector table.  Note that the proper constructs must be placed on this to */
 113:srcc/startup_msp432p401r_gcc.c **** /* ensure that it ends up at physical address 0x0000.0000 or at the start of          */
 114:srcc/startup_msp432p401r_gcc.c **** /* the program if located at a start address other than 0.                            */
 115:srcc/startup_msp432p401r_gcc.c **** void (* const interruptVectors[])(void) __attribute__ ((section (".intvecs"))) =
 116:srcc/startup_msp432p401r_gcc.c **** {
 117:srcc/startup_msp432p401r_gcc.c ****     (pFunc)&__StackTop,
 118:srcc/startup_msp432p401r_gcc.c ****                                            /* The initial stack pointer */
 119:srcc/startup_msp432p401r_gcc.c ****     Reset_Handler,                         /* The reset handler         */
 120:srcc/startup_msp432p401r_gcc.c ****     NMI_Handler,                           /* The NMI handler           */
 121:srcc/startup_msp432p401r_gcc.c ****     HardFault_Handler,                     /* The hard fault handler    */
 122:srcc/startup_msp432p401r_gcc.c ****     MemManage_Handler,                     /* The MPU fault handler     */
 123:srcc/startup_msp432p401r_gcc.c ****     BusFault_Handler,                      /* The bus fault handler     */
 124:srcc/startup_msp432p401r_gcc.c ****     UsageFault_Handler,                    /* The usage fault handler   */
 125:srcc/startup_msp432p401r_gcc.c ****     0,                                     /* Reserved                  */
 126:srcc/startup_msp432p401r_gcc.c ****     0,                                     /* Reserved                  */
 127:srcc/startup_msp432p401r_gcc.c ****     0,                                     /* Reserved                  */
 128:srcc/startup_msp432p401r_gcc.c ****     0,                                     /* Reserved                  */
 129:srcc/startup_msp432p401r_gcc.c **** 	SVC_Handler,                           /* SVCall handler            */
 130:srcc/startup_msp432p401r_gcc.c ****     DebugMon_Handler,                      /* Debug monitor handler     */
 131:srcc/startup_msp432p401r_gcc.c ****     0,                                     /* Reserved                  */
 132:srcc/startup_msp432p401r_gcc.c **** 	PendSV_Handler,                        /* The PendSV handler        */
 133:srcc/startup_msp432p401r_gcc.c ****     SysTick_Handler,                       /* The SysTick handler15       */
 134:srcc/startup_msp432p401r_gcc.c ****     PSS_IRQHandler,                        /* PSS ISR                   */
 135:srcc/startup_msp432p401r_gcc.c ****     CS_IRQHandler,                         /* CS ISR                    */
 136:srcc/startup_msp432p401r_gcc.c ****     PCM_IRQHandler,                        /* PCM ISR                   */
 137:srcc/startup_msp432p401r_gcc.c ****     WDT_A_IRQHandler,                      /* WDT ISR                   */
 138:srcc/startup_msp432p401r_gcc.c ****     FPU_IRQHandler,                        /* FPU ISR                   */
 139:srcc/startup_msp432p401r_gcc.c ****     FLCTL_IRQHandler,                      /* FLCTL ISR                 */
 140:srcc/startup_msp432p401r_gcc.c ****     COMP_E0_IRQHandler,                    /* COMP0 ISR                 */
 141:srcc/startup_msp432p401r_gcc.c ****     COMP_E1_IRQHandler,                    /* COMP1 ISR                 */
 142:srcc/startup_msp432p401r_gcc.c ****     TA0_0_IRQHandler,                      /* TA0_0 ISR                 */
 143:srcc/startup_msp432p401r_gcc.c ****     TA0_N_IRQHandler,                      /* TA0_N ISR                 */
 144:srcc/startup_msp432p401r_gcc.c ****     TA1_0_IRQHandler,                      /* TA1_0 ISR                 */
 145:srcc/startup_msp432p401r_gcc.c ****     TA1_N_IRQHandler,                      /* TA1_N ISR                 */
 146:srcc/startup_msp432p401r_gcc.c ****     TA2_0_IRQHandler,                      /* TA2_0 ISR                 */
 147:srcc/startup_msp432p401r_gcc.c ****     TA2_N_IRQHandler,                      /* TA2_N ISR                 */
 148:srcc/startup_msp432p401r_gcc.c ****     TA3_0_IRQHandler,                      /* TA3_0 ISR                 */
 149:srcc/startup_msp432p401r_gcc.c ****     TA3_N_IRQHandler,                      /* TA3_N ISR                 */
 150:srcc/startup_msp432p401r_gcc.c **** 	EUSCIA0_IRQHandler,                   /* EUSCIA0 ISR写1擦除，user程序不可使用*/
 151:srcc/startup_msp432p401r_gcc.c ****     EUSCIA1_IRQHandler,                    /* EUSCIA1 ISR               */
 152:srcc/startup_msp432p401r_gcc.c ****     EUSCIA2_IRQHandler,                    /* EUSCIA2 ISR               */
 153:srcc/startup_msp432p401r_gcc.c ****     EUSCIA3_IRQHandler,                    /* EUSCIA3 ISR               */
 154:srcc/startup_msp432p401r_gcc.c ****     EUSCIB0_IRQHandler,                    /* EUSCIB0 ISR               */
 155:srcc/startup_msp432p401r_gcc.c ****     EUSCIB1_IRQHandler,                    /* EUSCIB1 ISR               */
 156:srcc/startup_msp432p401r_gcc.c ****     EUSCIB2_IRQHandler,                    /* EUSCIB2 ISR               */
 157:srcc/startup_msp432p401r_gcc.c ****     EUSCIB3_IRQHandler,                    /* EUSCIB3 ISR               */
 158:srcc/startup_msp432p401r_gcc.c ****     ADC14_IRQHandler,                      /* ADC14 ISR                 */
 159:srcc/startup_msp432p401r_gcc.c **** 	T32_INT1_IRQHandler,                   /* T32_INT1 ISR写1擦除，user程序不可使用*/
 160:srcc/startup_msp432p401r_gcc.c ****     T32_INT2_IRQHandler,                   /* T32_INT2 ISR              */
 161:srcc/startup_msp432p401r_gcc.c ****     T32_INTC_IRQHandler,                   /* T32_INTC ISR              */
 162:srcc/startup_msp432p401r_gcc.c ****     AES256_IRQHandler,                     /* AES ISR                   */
 163:srcc/startup_msp432p401r_gcc.c ****     RTC_C_IRQHandler,                      /* RTC ISR                   */
 164:srcc/startup_msp432p401r_gcc.c ****     DMA_ERR_IRQHandler,                    /* DMA_ERR ISR               */
 165:srcc/startup_msp432p401r_gcc.c ****     DMA_INT3_IRQHandler,                   /* DMA_INT3 ISR              */
 166:srcc/startup_msp432p401r_gcc.c ****     DMA_INT2_IRQHandler,                   /* DMA_INT2 ISR              */
 167:srcc/startup_msp432p401r_gcc.c ****     DMA_INT1_IRQHandler,                   /* DMA_INT1 ISR              */
 168:srcc/startup_msp432p401r_gcc.c ****     DMA_INT0_IRQHandler,                   /* DMA_INT0 ISR              */
 169:srcc/startup_msp432p401r_gcc.c ****     PORT1_IRQHandler,                      /* PORT1 ISR                 */
 170:srcc/startup_msp432p401r_gcc.c ****     PORT2_IRQHandler,                      /* PORT2 ISR                 */
 171:srcc/startup_msp432p401r_gcc.c ****     PORT3_IRQHandler,                      /* PORT3 ISR                 */
 172:srcc/startup_msp432p401r_gcc.c ****     PORT4_IRQHandler,                      /* PORT4 ISR                 */
 173:srcc/startup_msp432p401r_gcc.c ****     PORT5_IRQHandler,                      /* PORT5 ISR                 */
 174:srcc/startup_msp432p401r_gcc.c ****     PORT6_IRQHandler                       /* PORT6 ISR                 */
 175:srcc/startup_msp432p401r_gcc.c **** };
 176:srcc/startup_msp432p401r_gcc.c **** 
 177:srcc/startup_msp432p401r_gcc.c **** /* Forward declaration of the default fault handlers. */
 178:srcc/startup_msp432p401r_gcc.c **** /* This is the code that gets called when the processor first starts execution */
 179:srcc/startup_msp432p401r_gcc.c **** /* following a reset event.  Only the absolutely necessary set is performed,   */
 180:srcc/startup_msp432p401r_gcc.c **** /* after which the application supplied entry() routine is called.  Any fancy  */
 181:srcc/startup_msp432p401r_gcc.c **** /* actions (such as making decisions based on the reset cause register, and    */
 182:srcc/startup_msp432p401r_gcc.c **** /* resetting the bits in that register) are left solely in the hands of the    */
 183:srcc/startup_msp432p401r_gcc.c **** /* application.                                                                */
 184:srcc/startup_msp432p401r_gcc.c **** void Reset_Handler(void)
 185:srcc/startup_msp432p401r_gcc.c **** {
  92              		.loc 1 185 0
  93              		.cfi_startproc
  94              		@ args = 0, pretend = 0, frame = 8
  95              		@ frame_needed = 1, uses_anonymous_args = 0
  96 0000 80B5     		push	{r7, lr}
  97              		.cfi_def_cfa_offset 8
  98              		.cfi_offset 7, -8
  99              		.cfi_offset 14, -4
 100 0002 82B0     		sub	sp, sp, #8
 101              		.cfi_def_cfa_offset 16
 102 0004 00AF     		add	r7, sp, #0
 103              		.cfi_def_cfa_register 7
 186:srcc/startup_msp432p401r_gcc.c **** 	/* Copy the data segment initializers from flash to SRAM. */
 187:srcc/startup_msp432p401r_gcc.c **** 	    uint32_t *pui32Src, *pui32Dest;
 188:srcc/startup_msp432p401r_gcc.c **** 
 189:srcc/startup_msp432p401r_gcc.c **** 	    pui32Src = &__data_load__;
 104              		.loc 1 189 0
 105 0006 124B     		ldr	r3, .L4
 106 0008 7B60     		str	r3, [r7, #4]
 190:srcc/startup_msp432p401r_gcc.c **** 	    for(pui32Dest = &__data_start__; pui32Dest < &__data_end__; )
 107              		.loc 1 190 0
 108 000a 124B     		ldr	r3, .L4+4
 109 000c 3B60     		str	r3, [r7]
 110 000e 07E0     		b	.L2
 111              	.L3:
 191:srcc/startup_msp432p401r_gcc.c **** 	    {
 192:srcc/startup_msp432p401r_gcc.c **** 	        *pui32Dest++ = *pui32Src++;
 112              		.loc 1 192 0
 113 0010 7A68     		ldr	r2, [r7, #4]
 114 0012 131D     		adds	r3, r2, #4
 115 0014 7B60     		str	r3, [r7, #4]
 116 0016 3B68     		ldr	r3, [r7]
 117 0018 191D     		adds	r1, r3, #4
 118 001a 3960     		str	r1, [r7]
 119 001c 1268     		ldr	r2, [r2]
 120 001e 1A60     		str	r2, [r3]
 121              	.L2:
 190:srcc/startup_msp432p401r_gcc.c **** 	    for(pui32Dest = &__data_start__; pui32Dest < &__data_end__; )
 122              		.loc 1 190 0
 123 0020 3B68     		ldr	r3, [r7]
 124 0022 0D4A     		ldr	r2, .L4+8
 125 0024 9342     		cmp	r3, r2
 126 0026 F3D3     		bcc	.L3
 193:srcc/startup_msp432p401r_gcc.c **** 	    }
 194:srcc/startup_msp432p401r_gcc.c **** 
 195:srcc/startup_msp432p401r_gcc.c **** 	    /* Zero fill the bss segment. */
 196:srcc/startup_msp432p401r_gcc.c **** 	    __asm("    ldr     r0, =__bss_start__\n"
 127              		.loc 1 196 0
 128              		.syntax unified
 129              	@ 196 "srcc/startup_msp432p401r_gcc.c" 1
 130 0028 0E48     		    ldr     r0, =__bss_start__
 131 002a 0F49     	    ldr     r1, =__bss_end__
 132 002c 4FF00002 	    mov     r2, #0
 133              	    .thumb_func
 134              	zero_loop:
 135 0030 8842     	    cmp     r0, r1
 136 0032 B8BF     	    it      lt
 137 0034 40F8042B 	    strlt   r2, [r0], #4
 138 0038 FADB     	    blt     zero_loop
 139              	@ 0 "" 2
 197:srcc/startup_msp432p401r_gcc.c **** 	          "    ldr     r1, =__bss_end__\n"
 198:srcc/startup_msp432p401r_gcc.c **** 	          "    mov     r2, #0\n"
 199:srcc/startup_msp432p401r_gcc.c **** 	          "    .thumb_func\n"
 200:srcc/startup_msp432p401r_gcc.c **** 	          "zero_loop:\n"
 201:srcc/startup_msp432p401r_gcc.c **** 	          "    cmp     r0, r1\n"
 202:srcc/startup_msp432p401r_gcc.c **** 	          "    it      lt\n"
 203:srcc/startup_msp432p401r_gcc.c **** 	          "    strlt   r2, [r0], #4\n"
 204:srcc/startup_msp432p401r_gcc.c **** 	          "    blt     zero_loop");
 205:srcc/startup_msp432p401r_gcc.c **** 	    /* Call the application's entry point. */
 206:srcc/startup_msp432p401r_gcc.c **** 		SystemInit();
 140              		.loc 1 206 0
 141              		.thumb
 142              		.syntax unified
 143 003a FFF7FEFF 		bl	SystemInit
 207:srcc/startup_msp432p401r_gcc.c **** 	    Vectors_Init();  //User中使用BIOS区域构件函数指针初始化
 144              		.loc 1 207 0
 145 003e FFF7FEFF 		bl	Vectors_Init
 208:srcc/startup_msp432p401r_gcc.c **** //        uart_init(UART_Debug,115200);
 209:srcc/startup_msp432p401r_gcc.c **** //        uart_enable_re_int(UART_Debug);
 210:srcc/startup_msp432p401r_gcc.c **** 	    main();
 146              		.loc 1 210 0
 147 0042 FFF7FEFF 		bl	main
 211:srcc/startup_msp432p401r_gcc.c **** }
 148              		.loc 1 211 0
 149 0046 00BF     		nop
 150 0048 0837     		adds	r7, r7, #8
 151              		.cfi_def_cfa_offset 8
 152 004a BD46     		mov	sp, r7
 153              		.cfi_def_cfa_register 13
 154              		@ sp needed
 155 004c 80BD     		pop	{r7, pc}
 156              	.L5:
 157 004e 00BF     		.align	2
 158              	.L4:
 159 0050 00000000 		.word	__data_load__
 160 0054 00000000 		.word	__data_start__
 161 0058 00000000 		.word	__data_end__
 162              		.cfi_endproc
 163              	.LFE123:
 165              		.align	1
 166              		.global	Default_Handler
 167              		.syntax unified
 168              		.thumb
 169              		.thumb_func
 170              		.fpu fpv4-sp-d16
 172              	Default_Handler:
 173              	.LFB124:
 212:srcc/startup_msp432p401r_gcc.c **** 
 213:srcc/startup_msp432p401r_gcc.c **** /* This is the code that gets called when the processor receives an unexpected  */
 214:srcc/startup_msp432p401r_gcc.c **** /* interrupt.  This simply enters an infinite loop, preserving the system state */
 215:srcc/startup_msp432p401r_gcc.c **** /* for examination by a debugger.                                               */
 216:srcc/startup_msp432p401r_gcc.c **** void Default_Handler(void)
 217:srcc/startup_msp432p401r_gcc.c **** {
 174              		.loc 1 217 0
 175              		.cfi_startproc
 176              		@ args = 0, pretend = 0, frame = 0
 177              		@ frame_needed = 1, uses_anonymous_args = 0
 178              		@ link register save eliminated.
 179 005c 80B4     		push	{r7}
 180              		.cfi_def_cfa_offset 4
 181              		.cfi_offset 7, -4
 182 005e 00AF     		add	r7, sp, #0
 183              		.cfi_def_cfa_register 7
 184              	.L7:
 218:srcc/startup_msp432p401r_gcc.c **** 	/* Enter an infinite loop. */
 219:srcc/startup_msp432p401r_gcc.c **** 	while(1)
 185              		.loc 1 219 0
 186 0060 FEE7     		b	.L7
 187              		.cfi_endproc
 188              	.LFE124:
 190              		.weak	PORT6_IRQHandler
 191              		.thumb_set PORT6_IRQHandler,Default_Handler
 192              		.weak	PORT5_IRQHandler
 193              		.thumb_set PORT5_IRQHandler,Default_Handler
 194              		.weak	PORT4_IRQHandler
 195              		.thumb_set PORT4_IRQHandler,Default_Handler
 196              		.weak	PORT3_IRQHandler
 197              		.thumb_set PORT3_IRQHandler,Default_Handler
 198              		.weak	PORT2_IRQHandler
 199              		.thumb_set PORT2_IRQHandler,Default_Handler
 200              		.weak	PORT1_IRQHandler
 201              		.thumb_set PORT1_IRQHandler,Default_Handler
 202              		.weak	DMA_INT0_IRQHandler
 203              		.thumb_set DMA_INT0_IRQHandler,Default_Handler
 204              		.weak	DMA_INT1_IRQHandler
 205              		.thumb_set DMA_INT1_IRQHandler,Default_Handler
 206              		.weak	DMA_INT2_IRQHandler
 207              		.thumb_set DMA_INT2_IRQHandler,Default_Handler
 208              		.weak	DMA_INT3_IRQHandler
 209              		.thumb_set DMA_INT3_IRQHandler,Default_Handler
 210              		.weak	DMA_ERR_IRQHandler
 211              		.thumb_set DMA_ERR_IRQHandler,Default_Handler
 212              		.weak	RTC_C_IRQHandler
 213              		.thumb_set RTC_C_IRQHandler,Default_Handler
 214              		.weak	AES256_IRQHandler
 215              		.thumb_set AES256_IRQHandler,Default_Handler
 216              		.weak	T32_INTC_IRQHandler
 217              		.thumb_set T32_INTC_IRQHandler,Default_Handler
 218              		.weak	T32_INT2_IRQHandler
 219              		.thumb_set T32_INT2_IRQHandler,Default_Handler
 220              		.weak	T32_INT1_IRQHandler
 221              		.thumb_set T32_INT1_IRQHandler,Default_Handler
 222              		.weak	ADC14_IRQHandler
 223              		.thumb_set ADC14_IRQHandler,Default_Handler
 224              		.weak	EUSCIB3_IRQHandler
 225              		.thumb_set EUSCIB3_IRQHandler,Default_Handler
 226              		.weak	EUSCIB2_IRQHandler
 227              		.thumb_set EUSCIB2_IRQHandler,Default_Handler
 228              		.weak	EUSCIB1_IRQHandler
 229              		.thumb_set EUSCIB1_IRQHandler,Default_Handler
 230              		.weak	EUSCIB0_IRQHandler
 231              		.thumb_set EUSCIB0_IRQHandler,Default_Handler
 232              		.weak	EUSCIA3_IRQHandler
 233              		.thumb_set EUSCIA3_IRQHandler,Default_Handler
 234              		.weak	EUSCIA2_IRQHandler
 235              		.thumb_set EUSCIA2_IRQHandler,Default_Handler
 236              		.weak	EUSCIA1_IRQHandler
 237              		.thumb_set EUSCIA1_IRQHandler,Default_Handler
 238              		.weak	EUSCIA0_IRQHandler
 239              		.thumb_set EUSCIA0_IRQHandler,Default_Handler
 240              		.weak	TA3_N_IRQHandler
 241              		.thumb_set TA3_N_IRQHandler,Default_Handler
 242              		.weak	TA3_0_IRQHandler
 243              		.thumb_set TA3_0_IRQHandler,Default_Handler
 244              		.weak	TA2_N_IRQHandler
 245              		.thumb_set TA2_N_IRQHandler,Default_Handler
 246              		.weak	TA2_0_IRQHandler
 247              		.thumb_set TA2_0_IRQHandler,Default_Handler
 248              		.weak	TA1_N_IRQHandler
 249              		.thumb_set TA1_N_IRQHandler,Default_Handler
 250              		.weak	TA1_0_IRQHandler
 251              		.thumb_set TA1_0_IRQHandler,Default_Handler
 252              		.weak	TA0_N_IRQHandler
 253              		.thumb_set TA0_N_IRQHandler,Default_Handler
 254              		.weak	TA0_0_IRQHandler
 255              		.thumb_set TA0_0_IRQHandler,Default_Handler
 256              		.weak	COMP_E1_IRQHandler
 257              		.thumb_set COMP_E1_IRQHandler,Default_Handler
 258              		.weak	COMP_E0_IRQHandler
 259              		.thumb_set COMP_E0_IRQHandler,Default_Handler
 260              		.weak	FLCTL_IRQHandler
 261              		.thumb_set FLCTL_IRQHandler,Default_Handler
 262              		.weak	FPU_IRQHandler
 263              		.thumb_set FPU_IRQHandler,Default_Handler
 264              		.weak	WDT_A_IRQHandler
 265              		.thumb_set WDT_A_IRQHandler,Default_Handler
 266              		.weak	PCM_IRQHandler
 267              		.thumb_set PCM_IRQHandler,Default_Handler
 268              		.weak	CS_IRQHandler
 269              		.thumb_set CS_IRQHandler,Default_Handler
 270              		.weak	PSS_IRQHandler
 271              		.thumb_set PSS_IRQHandler,Default_Handler
 272              		.weak	SysTick_Handler
 273              		.thumb_set SysTick_Handler,Default_Handler
 274              		.weak	PendSV_Handler
 275              		.thumb_set PendSV_Handler,Default_Handler
 276              		.weak	DebugMon_Handler
 277              		.thumb_set DebugMon_Handler,Default_Handler
 278              		.weak	SVC_Handler
 279              		.thumb_set SVC_Handler,Default_Handler
 280              		.weak	UsageFault_Handler
 281              		.thumb_set UsageFault_Handler,Default_Handler
 282              		.weak	BusFault_Handler
 283              		.thumb_set BusFault_Handler,Default_Handler
 284              		.weak	MemManage_Handler
 285              		.thumb_set MemManage_Handler,Default_Handler
 286              		.weak	HardFault_Handler
 287              		.thumb_set HardFault_Handler,Default_Handler
 288              		.weak	NMI_Handler
 289              		.thumb_set NMI_Handler,Default_Handler
 290              	.Letext0:
 291              		.file 2 "d:\\ahl-gec-ide(4.20)\\gcc\\arm-none-eabi\\include\\machine\\_default_types.h"
 292              		.file 3 "d:\\ahl-gec-ide(4.20)\\gcc\\arm-none-eabi\\include\\sys\\_stdint.h"
 293              		.file 4 "C:\\Users\\lenovo\\Desktop\\MSP-20210417\\MSP-20210417\\User-MSP432-20210417\\ch11-SPI-CT
 294              		.file 5 "C:\\Users\\lenovo\\Desktop\\MSP-20210417\\MSP-20210417\\User-MSP432-20210417\\ch11-SPI-CT
 295              		.file 6 "C:\\Users\\lenovo\\Desktop\\MSP-20210417\\MSP-20210417\\User-MSP432-20210417\\ch11-SPI-CT
 296              		.file 7 "d:\\ahl-gec-ide(4.20)\\gcc\\arm-none-eabi\\include\\sys\\lock.h"
 297              		.file 8 "d:\\ahl-gec-ide(4.20)\\gcc\\arm-none-eabi\\include\\sys\\_types.h"
 298              		.file 9 "d:\\ahl-gec-ide(4.20)\\gcc\\lib\\gcc\\arm-none-eabi\\7.2.1\\include\\stddef.h"
 299              		.file 10 "d:\\ahl-gec-ide(4.20)\\gcc\\arm-none-eabi\\include\\sys\\reent.h"
 300              		.file 11 "C:\\Users\\lenovo\\Desktop\\MSP-20210417\\MSP-20210417\\User-MSP432-20210417\\ch11-SPI-C
 301              		.file 12 "C:\\Users\\lenovo\\Desktop\\MSP-20210417\\MSP-20210417\\User-MSP432-20210417\\ch11-SPI-C
DEFINED SYMBOLS
                            *ABS*:00000000 startup_msp432p401r_gcc.c
                            *COM*:00000004 component_fun
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:23     .intvecs:00000000 interruptVectors
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:20     .intvecs:00000000 $d
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:89     .text:00000000 Reset_Handler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c NMI_Handler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c HardFault_Handler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c MemManage_Handler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c BusFault_Handler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c UsageFault_Handler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c SVC_Handler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c DebugMon_Handler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c PendSV_Handler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c SysTick_Handler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c PSS_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c CS_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c PCM_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c WDT_A_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c FPU_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c FLCTL_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c COMP_E0_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c COMP_E1_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c TA0_0_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c TA0_N_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c TA1_0_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c TA1_N_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c TA2_0_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c TA2_N_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c TA3_0_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c TA3_N_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c EUSCIA0_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c EUSCIA1_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c EUSCIA2_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c EUSCIA3_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c EUSCIB0_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c EUSCIB1_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c EUSCIB2_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c EUSCIB3_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c ADC14_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c T32_INT1_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c T32_INT2_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c T32_INTC_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c AES256_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c RTC_C_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c DMA_ERR_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c DMA_INT3_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c DMA_INT2_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c DMA_INT1_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c DMA_INT0_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c PORT1_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c PORT2_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c PORT3_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c PORT4_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c PORT5_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c PORT6_IRQHandler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:82     .text:00000000 $t
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:134    .text:00000030 zero_loop
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:159    .text:00000050 $d
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:165    .text:0000005c $t
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:172    .text:0000005c Default_Handler
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:302    .text:00000062 $d
C:\Users\lenovo\AppData\Local\Temp\cct5P5RM.s:2462   .text:00000064 $d

UNDEFINED SYMBOLS
__StackTop
__bss_start__
__bss_end__
SystemInit
Vectors_Init
main
__data_load__
__data_start__
__data_end__
